Light Diesel Vehicles

|  |
| --- |
| Required |
|  |
| Battery |
|  |
| Required |
|  |
| Ensure the battery is secure, clean, and free from corrosion |
|  |
| Other |
| ShowHide |
|  |
| Belts |
|  |
| Required |
|  |
| Check condition of fan, AC, and alternator belts - Ensure no wear or cracking |
|  |
| Other |
| ShowHide |
|  |
| Brakes |
|  |
| Required |
|  |
| Check brake pads & parking brake - Inspect for wear, top-up brake fluid if necessary. |
|  |
| Other |
| ShowHide |
|  |
| Emergency Response Card |
|  |
| Required |
|  |
| Confirm card is present & legible |
|  |
| Other |
| ShowHide |
|  |
| Fire Extinguisher (if fitted) |
|  |
|  |
| Ensure presence, ease of access, test status and condition |
|  |
| Other |
| ShowHide |
|  |
| First Aid Kit |
|  |
| Required |
|  |
| Ensure kit is present, fully stocked and easily accessible. Check items are within expiry dates |
|  |
| Other |
| ShowHide |
|  |
| General Safety |
|  |
| Required |
|  |
| Ensure the vehicle is free from hazards and deemed safe to operate |
|  |
| Light ndiesel vehicles |
| ShowHide |
|  |
| Lights |
|  |
| Required |
|  |
| Ensure all lights are functional - Tail lights, indicators, head lights & flashing lights |
|  |
| Other |
| ShowHide |
|  |
| Oil |
|  |
| Required |
|  |
| Check engine oil, transmission oil, power steering oil - top up as required |
|  |
| Other |
| ShowHide |
|  |
| Presentation & Cleanliness |
|  |
| Required |
|  |
| Inspect the vehicle for cleanliness and presentability |
|  |
| Other |
| ShowHide |
|  |
| Radiator (Coolant) |
|  |
| Required |
|  |
| Check coolant levels and condition |
|  |
| Other |
| ShowHide |
|  |
| Registration |
|  |
| Required |
|  |
| Check registration label is current |
|  |
| Other |
| ShowHide |
|  |
| Road User Charges (RUC) |
|  |
| Required |
|  |
| Check RUC label is current |
|  |
| Other |
| ShowHide |
|  |
| Seatbelt |
|  |
| Required |
|  |
| Check condition and functionality - ensure belts are secured and not frayed |
|  |
| Other |
| ShowHide |
|  |
| Tyres/Wheels |
|  |
| Required |
|  |
| Inspect for visual wear or damage, ensure proper inflation |
|  |
| Other |
| ShowHide |
|  |
| Warning Devices |
|  |
| Required |
|  |
| Check horn, reversing beeper, and audible alarms to ensure they function properly |
|  |
| Other |
| ShowHide |
|  |
| Warrant of Fitness (WOF) |
|  |
| Required |
|  |
| Check WOF is current |
|  |
| Other |
| ShowHide |
|  |
| Windscreen, Windows & Mirrors |
|  |
| Required |
|  |
| Check condition and clarity of windows & mirrors |
|  |
| Check wiper blade condition & replace as necessary |
|  |
| Check wiper fluid & top up as necessary |
|  |
| Other |